# UPC-EAN.SUPPLEMENT

UPC/EAN Supplementals. The cmbSDK's mobile camera API only supports turning UPC/EAN supplement code support on/off, while the DMCC command allows them to be off, required, require a 2 digit, require a 5 digit, or optionally permit them. The cmbSDK's mobile camera API will treat options 1-4 the same; to simply enable them.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
option | enum | [0-4] | 0: Ignore 1: Required 2: Required 2 digit 3: Required 5 digit 4: Not required

## Platforms

ALL

## Notes

Version: 3.0.0