# CAMERA.INTERVAL-US

The acquisition interval, the time between successive camera acquisitions in microseconds. Supported with Burst, Self, and Continuous trigger types.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
us | int | [*-1000000] | Microseconds. Step size is 250. * By default the minimum range is 6000 but this can change depending on decode timeout and field of view.

## Platforms

DM50, DM60, DM70, DM280, DM300, DM360, DM370, DM470, DM503

## Notes

Version: 4.0.0