View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 150

DataMan 260

DataMan 280

DataMan 300

DataMan 360

DataMan 370

DataMan 470

DataMan 503

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# Which trigger modes are Read Setups valid for?

Read Setups can be used in Single, Self, Burst, and Continuous trigger modes. The next Read Setup becomes active after the specified Interval time (specified on the Optimize Image pane). For all other trigger modes, if multiple setups have been configured, only the currently selected active setup (indicated in status bar) gets used. Because there is no interval for Single trigger mode, one read setup will go to the next one as soon as the previous acquisition finishes.

Note: default,DM050,DM060,DM070,DM150,DM260,DM300,DM360, DM370,DM280, DM470, DM503