View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 150

DataMan 260

DataMan 280

DataMan 300

DataMan 360

DataMan 370

DataMan 470

DataMan 503

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# How do I set a longer burst length?

The maximum burst length you can specify depends on the resources available on the device. By default, the maximum burst length is 120 images, but you can enhance this by increasing the memory to store images captured by the reader. Increase the memory available for storing burst images by unreserving the image slots which are currently dedicated to image lift and by decreasing the size of the imager field of view. This can be done through the Image Size (Region of Interest) pane:

1. Select the Image Size (Region of Interest) pane.
2. Check the Imager FoV check box (in Single, Burst, and Continuous trigger modes) and reduce the size of the Imager FoV.

Once reduced, you can increase the Burst length parameter in the Application Details step.

Note: DM503