View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 150

DataMan 260

DataMan 280

DataMan 300

DataMan 360

DataMan 370

DataMan 470

DataMan 503

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# What is the difference between the After First Read and After Last Read Delay option?

The After First Read delay starts timing after the first time a given code is read, and the timer will not reset. This means that a code may be re-read if the reader is triggered in a multiple-image mode such as Continuous, and if the code is in front of the reader for an amount of time equal to or exceeding the Re-Read Delay.

After Last Read resets the timer every time a given code appears in an image. This means that the code will not re-read, as long as it stays in front of the reader. Only removing the code from the reader's field of view for a time equal to or exceeding the Re-Read Delay will cause the code to re-read.

Note: DM050,DM060,DM070,DM260,DM300,DM360, DM370,DM280, DM470, DM503,DM8050,DM8070,DM8600