View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 150

DataMan 260

DataMan 280

DataMan 300

DataMan 360

DataMan 370

DataMan 470

DataMan 503

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# What is the RTM Lean device that shows up under Network?

Real Time Monitoring (RTM) Lean is a feature built into DataMan Setup Tool that allows for the collection and analysis of different kinds of data related to devices on the network and their readings. You can connect to RTM Lean as you would to a device, then proceed to set up data collection in a newly opened document. RTM Lean only collects data actively when running and you are connected to it.

During the initial setup, you are asked to choose the device that RTM Lean is going to monitor, and then what kind of data (outside of the default) it is going to collect. This can be redefined under Configuration on the ribbon menu. By default, RTM Lean collects statistical data (Read Rate, trigger count, trigger overrun, buffer overflow, and process control metrics, if enabled on the device).

NOTE: RTM Lean can acquire data from a single device at a time and keep data for 48 hours.

Note: DM050,DM060,DM070,DM150,DM260,DM300,DM360, DM370,DM280, DM470, DM503,DM8050,DM8070,DM8600,DM8700,MX-1000,MX-1500