View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 150

DataMan 260

DataMan 280

DataMan 300

DataMan 360

DataMan 370

DataMan 470

DataMan 503

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# What is distance based Secondary Reader Response Timeout?

The Secondary Reader Response Timeout has a distance based mode for applications implementing distance based trigger delays. In distance based mode, the Secondary Reader Response Timeout is the distance in millimeters that triggers a primary-secondary timeout response.

Note: DM060,DM070,DM260,DM300,DM360, DM370,DM280, DM470, DM503