View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 150

DataMan 260

DataMan 280

DataMan 300

DataMan 360

DataMan 370

DataMan 470

DataMan 503

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# What system settings can I change?

You can disable or enable the beeper.

The System Settings drop-down list on the Advanced tab lets you control what the reader does when it reads a code, when it cannot read a code and when it reads a code that fails validation.

- Sound level controls the pitch of the signal tone.

- Number of tones controls how many times the signal is sounded.

- LED color sets the color displayed by the reader's status indicator (mounted on the back of the reader).

- Enable vibration controls if a good read is signaled by vibration.

Note: MX-1000,MX-1500,DM8050,DM8070,DM8600,DM8700