View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 150

DataMan 260

DataMan 280

DataMan 300

DataMan 360

DataMan 370

DataMan 470

DataMan 503

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# How do I calculate the Interval value for Self and Continuous trigger modes?

The Interval Assistant helps you calculate this data. Click Interval Assistant for an easier and assisted way.

Because the Self and Continuous trigger modes can be used for moving applications, it is necessary to determine the correct interval time to capture the desired length of the part as it moves under the camera. The variables necessary for this calculation are:

1. Line speed in mm per second

2. Code size w/quiet zone in mm

3. FOV = Field of View (x or y) in mm

You can then use the following equation to determine the approximate interval time:

Interval = 1000 * ((FOV – 2(Code Size)) / Line Speed)

The (2 * Code Size) variable allows for overlap of the frames taken. This takes into consideration the condition where the code is slightly out of the field of view in one frame (acquisition). The (2 * Code Size) will overlap the field of view between successive frames and allow the code to be viewed in the field of view of the next frame.

Note: DM050,DM060,DM070,DM150,DM260,DM300,DM360, DM370,DM280, DM470, DM503