View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 150

DataMan 260

DataMan 280

DataMan 300

DataMan 360

DataMan 370

DataMan 470

DataMan 503

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# How do I configure the network settings of the reader?

If you are using a wireless DataMan 8000 reader, configure network settings on the base station. If you are using a tethered reader, use the Network tab to configure network settings.

Select the Use DHCP Server option to have the reader assigned an IP address by a DHCP server (if one is available), or enter the network settings manually. Contact your network administrator for an appropriate value.

When you change the settings, the question "The changes made require reboot to take effect. Apply changes and reboot now?" pops up. Click Yes. If, for any reason, you click No, you can still apply the changes. Choose System->Save Settings and then reboot your reader.

Note: DMAE50,DM060,DM070,DM150,DM260,DM300,DM360, DM370,DM280, DM470, DM503,DM8050,DM8070,DM8600,DM8700