# Communication Settings

Serial Communication Settings
Variable | Type | Description
--- | --- | ---
Used Communication Channel | array |
Enable Multi-Port (RS-232 Sharing) | boolean |
Speed | array |
Parity | array |
Data Bits | integer |
Stop Bits | integer |
Rs232 Inter Character Delay | integer |

Ethernet Communication Settings
Variable | Type | Description
--- | --- | ---
Use DHCP Server | boolean |
Subnet Mask | string |
Default Gateway | string |
DNS Server | string |
Domain Name | string |

Custom Command Settings
Variable | Type | Description
--- | --- | ---
Serial Trigger | Enabled | boolean |
Trigger On | string |
Trigger Off | string |
Echo Commands | Enabled | boolean |
Command Header | string |
Command Footer | string |

Network Communication Settings
Variable | Type | Description
--- | --- | ---
Telnet Port | integer |
Authentication | Enabled | boolean |
Username | string |
Password | string |
Network Client | Enabled | boolean |
Host Address | string |
Host Port | integer |
Client Port | integer |
Protocol | array |
Connection Timeout (ms) | integer |
Reconnect Delay (ms) | integer |
Open Connection | array |
Close Connection | array |
Disconnect Delay (ms) | integer |

Industrial Protocol Communication Settings
Variable | Type | Description
--- | --- | ---
Ethernet/IP | boolean |
PROFINET | Enabled | boolean |
Use Name of Station | boolean |
Name of Station | string |
SLMP | Enabled | boolean |
IP Address | string |
Host Port [hex] | integer |
Timeout | integer |
Poll Interval [ms] | integer |
PLC Series | array |
Network Number | integer |
PC Number [hex] | integer |
Destination Module | array |
Control | Selected Device | array |
Number of Devices | integer |
Offset | integer |
Status | Selected Device | array |
Number of Devices | integer |
Offset | integer |
PLC Input | Selected Device | array |
Number of Devices | integer |
Offset | integer |
PLC Output | Selected Device | array |
Number of Devices | integer |
Offset | integer |
Command | Selected Device | array |
Number of Devices | integer |
Offset | integer |
Command Result | Selected Device | array |
Number of Devices | integer |
Offset | integer |
Modbus TCP | Enabled | boolean |
Port | integer |
Maximum Connections | integer |
Idle Timeout [s] | integer |
String Byte Swap | boolean |
Holding Register Only Mode | boolean |
Control | Address Space | array |
Offset | integer |
Quantity | integer |
Status | Address Space | array |
Offset | integer |
Quantity | integer |
PLC Input | Address Space | array |
Offset | integer |
Quantity | integer |
PLC Output | Address Space | array |
Offset | integer |
Quantity | integer |
Command | Address Space | array |
Offset | integer |
Quantity | integer |
Command Result | Address Space | array |
Offset | integer |
Quantity | integer |
Cc Link | boolean |
Iq Ss | Enabled | boolean |
Language | array |

Other Communication Settings
Variable | Type | Description
--- | --- | ---
Script | string |
Script Enabled | boolean |
Translate Unprintable Chars | boolean |
Wake-up Message | boolean |