# Connecting the Edge Intelligence

Unpack your Edge Intelligence unit and check that the following components have been included: power cable, display port to VGA adapter, and DIN rail mounting kit.

Perform the steps below before connecting to the web user interface:

1. Connect Edge Intelligence unit to your Enterprise network using the External Ethernet port.

   | EI-200 | EI-300 | EI-700
   1 | External (DHCP) | External (DHCP) | External (DHCP)
   2 | Internal (192.168.1.100) | Internal (192.168.1.100) | Internal (192.168.1.100)
   3 | N/A | Internal (DHCP default) | Internal (DHCP default)

2. Connect Edge Intelligence unit to your reader network LAN using the Internal Ethernet port.

3. Connect any desired peripherals such as monitor, mouse, or keyboard to your Edge Intelligence unit using the USB ports before powering on the device.

4. Connect Edge Intelligence unit to power and start the device.