# Edge Intelligence Systems

Edge Intelligence Model | CPU | Processing Power | Number of Data Streams | Power | I/O | Memory | Image Capacity1Assuming no-read images are saved at full resolution (3 megapixels) in JPEG format. | Image Storage2With full resolution JPEG no-read images from all readers, on a system running 24/7 with 1 trigger per second at a performance of 99% read rate.
EI-200 | Intel Celeron N3350 1.1 GHz | Dual Core | Up to 5 data streams | 12 VDC input jack | Not supported | 4 GB LLDDR4 2133 MHz | Up to 1 million images | Up to 244 data days
EI-300 | Intel Atom E3950 1.6 GHz | Quad Core | Up to 10 data streams | 9~36 VDC 3-pin terminal block | 8-bit Isolated Digital I/O | 8 GB LPDDR4 | Up to 4 million images | Up to 487 data days
EI-700 | Intel Core i7-8700T 2.4 GHz | Hexa Core | Up to 20 data streams | 9~48 VDC 5-pin terminal block | 8-bit Isolated Digital I/O | 8 GB SO-DIMM DDR4 2666 MHz - Wide Temp | Up to 8 million images | Up to 487 data days