# COM.USB-HID-ONLY

When enabled, the base station or the reader appears as a single USB Keyboard device on its USB port, instead of a composite device. The DM8000 base station G2 is supported from version 5.4.0, while DM8700 base station USB and DM8700 wired USB is supported from version 6.2.7.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
state | bool |  |

## Platforms

DM8000 base station G2, DM8700 base station USB, DM8700 wired USB

## Notes

Version: 5.4.0