# Set Event

Triggers a specified event in the EasyBuilder through a Native Mode command.

Note:

- If you configure the In-Sight vision system to accept an acquisition trigger from a PLC/Motion Controller through a Native Mode command, use the SetEvent and Wait function with the Event code set to 8 (SW8). This ensures that the vision system waits for both the acquisition and inspection to complete before sending a complete response back to the PLC/Motion Controller, and that previous inspection results are not being sent to the PLC/Motion Controller. You can also use the complete response from the vision system to create conditional PLC logic that sends a read request for the inspection results. For more information, see Set Event and Wait.

- If a PLC/Motion Controller uses the Set Event function to trigger an acquisition, the only way to use it is in cases where the inspection results are not also being read. Otherwise, the acquisition and the inspection are not in sync, with the vision system returning a response as soon as the image is acquired and before the inspection completes.

## Set Event Inputs

Syntax: SE<Int>

Parameter | Description
--- | ---
Int | The Event code to set. 0 to 7 = Specifies an external event (External 0, External 1 ... External 7). 8 = Acquires an image and updates the EasyBuilder. This option requires you to set the Trigger mode parameter of the AcquireImage function to Single.

## Set Event Outputs

Status Codes | Description
--- | ---
1 | The command execution is successful.
0 | Unrecognized command.
-1 | The number is either out of range (0 to 8) or not an integer.
-2 | The command execution is unsuccessful.
-6 | User does not have Full Access to execute the command.

## Set Event Example

You can use the SetEvent function to trigger events in the EasyBuilder through Native Mode commands.

The command to trigger External Event 0 is: SE0