# Filmstrip Window Components

The Filmstrip consists of the following parts:

Item | Name | Description
1 | Frames | The recorded frames, consisting of the following: Image Image name Sequence number The default frame name is Image. The sequence number of the frame is defined by the Counter. Double-clicking on the frame plays the frame back. Hovering over the name of the frame shows the location of the frame file and the date and time of recording. You can see two kinds of outlines around the frames: Blue Outline: Selection marker, indicates the user-selected frame or frames. Yellow Outline: Playback position marker, indicates the last played back frame on the filmstrip.
2 | Folder | Opens the Browse for Folder dialog where you can choose the location of the folder where the frames get saved or from where to load the frames. If you do not select any folder, the In-Sight 3D EasyBuilder saves the recorded frames to the following directory by default: <C>:\Documents\In-Sight Vision Suite\In-Sight\Filmstrip
3 | Frame name | Specifies the name of the frame. The default value is Image. To set a new frame name, type in a new name into the box.
4 | Counter | Specifies the sequence number of the frames. The Filmstrip automatically fills this field by counting the recorded or loaded frames. The value increases by one after each recording. You can overwrite this value by typing in a new number, or increasing/decreasing it by using the stepper buttons. The numbering starts from 0 and lasts until 9999. If the counter reaches 9999, counting restarts from 0. Overwriting the value means that the counting starts from the number you defined. For example, if you typed 50 into the box, the next recorded frame gets 50 as the sequence number, while the value of the counter increases to 51.
5 | File format | Shows the image file format for the recorded frames. For saving the image files, you can choose from .bmp, .jpg, or .png file formats. The default file format is .bmp.
6 | Record | You can record new images with this function. When the record mode is on, the button is blinking, indicating that the record function is ready for image acquisition. Clicking on the button again turns off the recording mode.
7 | Delay (ms) | Shows the time delay in milliseconds, meaning how fast one frame follows the next frame. The default value is 200 milliseconds. The minimum value is 0 ms, meaning there is no delay between the images during playback. The maximum value is 60 seconds (60 000 ms).
8 | Playback first frame | Click to play all frames back, starting from the first frame.
9 | Playback next frame | Click to play all frames back, starting from the currently selected or played back frame.
10 | Loop playback | Click to enable looped playback. Then click on the Playback next frame button to play back the frames in a loop. When the playback reaches the last frame of the filmstrip, the playback automatically restarts from the first frame. Click on the Stop button to finish the looped playback.
11 | Stop | Stops the playback of the filmstrip.
12 | Play First | Shows the first frame of the filmstrip.
13 | Play Previous | Shows the preceding frame before to the actual frame.
14 | Play Next | Shows the following frame after the actual frame.
15 | Play Last | Shows the last frame of the filmstrip.