# Bits du bloc d’état

Le bloc de bits État indique l’état actuel du système de vision.Le scanner SLMP met à jour le bloc de bits État une fois au démarrage du protocole, puis à chaque fois qu’un nouvel état est disponible. Le bloc de bis État est constitué de 112 bits. Certains bits sont réservés.

L’utilisation des bits du bloc État est récapitulée dans le tableau suivant. Ce tableau présente également les bits réservés.

Remarque : Pour obtenir une description détaillée des signaux, consultez la rubrique Signaux des communications industrielles.

Octet | Bit 7 | Bit 6 | Bit 5 | Bit 4 | Bit 3 | Bit 2 | Bit 1 | Bit 0
0 | Online |  |  | Acq Error | Réservé | Trigger Ack | Trigger Ready
1 | Error | Command Failed | Command Completed | Command Executing | Results Valid | Results Buffer Overrun | Inspection Completed |
2 | Réservé |  | Exposure Complete |  | String Command Ack | Set User Data Ack
3 | External Event Ack 7 | External Event Ack 6 | External Event Ack 5 | External Event Ack 4 | External Event Ack 3 | External Event Ack 2 | External Event Ack 1 | External Event Ack 0