# In-Sight 3800 Système de vision Table de référence du module E/S PROFINET

Cette rubrique fournit la table de référence du module E/S PROFINET, utilisable en conjonction avec le fichier GSD pour l’incorporation du système de vision In-Sight et d’un PLC Siemens via le protocole PROFINET.

Remarque : Pour obtenir des descriptions détaillées des signaux, consultez la rubrique Signaux des communications industrielles.

Module | ID | Octet | Bit 7 | Bit 6 | Bit 5 | Bit 4 | Bit 3 | Bit 2 | Bit 1 | Bit 0
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
Contrôle des acquisitions | 0x101 | 0 | Set Offline | Réservé | Clear Exposure Complete | Trigger | Trigger Enable
État des acquisitions | 0x201 | 0 | Online | Offline Reason | Acquisition Error | Exposure Complete | Trigger Acknowledge | Trigger Ready
1 | Réservé
2..3 | Acquisition ID
Contrôle de l’inspection | 0x102 | 0 | Clear Error | Réservé | Execute Command | Set User Data | Inspection Results Acknowledge | Buffer Results Enable
État des inspections | 0x203 | 0 | Set User Data Acknowledge | Command Failed | Command Completed | Command Executing | Results Valid | Results Buffer Overrun | Inspection Completed | Réservé
1 | Error | Réservé | Job Passed
2..3 | Error ID
Entrée de contrôle de commande | 0x108 | 0..1 | Command ID (16 bits)
Sortie de contrôle de commande | 0x108 | 0..1 | Current Job ID (16 bits)
2..3 | Command Result Code (16 bits)
Entrée de contrôle d’événement logiciel | 0x106 | 0 | External Event 7 | External Event 6 | External Event 5 | External Event 4 | External Event 3 | External Event 2 | External Event 1 | External Event 0
Sortie de contrôle d’événement externe | 0x106 | 0 | External Event Acknowledge 7 | External Event Acknowledge 6 | External Event Acknowledge 5 | External Event Acknowledge 4 | External Event Acknowledge 3 | External Event Acknowledge 2 | External Event Acknowledge 1 | External Event Acknowledge 0
User Data (jusqu’à 4 modules pour 1016 octets) | 0x301 (16) 0x302 (32) 0x303 (64) 0x304 (128) 0x305 (254) | 0..1015 max | User Data
Inspection Results (jusqu’à 4 modules pour 1000 octets) | 0x401 (16) 0x402 (32) 0x403 (64) 0x404 (128) 0x405 (250) | 0..1 | Inspection ID
2..3 | Inspection Results Code
4..1003 max | Inspection Results