# In-Sight® Device Pane

When initially launched, In-Sight Vision Suite automatically scans the network to discover and enumerate all of the detected In-Sight vision systems on the local subnet network. The devices are displayed in the In-Sight Device Pane, as seen below.

If the device does not appear in the list, you can manually add it. See the Configure Manual Devices topic for more information.

When a device is selected on the Device Pane, the following options become available:

Item | Menu | Description
1 | System Info | Shows information about the selected device. See the System Info topic for more information on the data displayed by this option.
2 | Connect | Connects to the selected device and launches the adapter to either program the device, or view the configured vision application running on it. See the Connect topic for more information.
3 | Open HMI | Opens a Web Browser connection to the selected device. In-Sight Vision Suite supports displaying an HMI on an Internet Web Browser, using Google Chrome. See the Open HMI topic for more information. Note: For more information about configuring and setting up an HMI in the adapter, see the WebPages topics in the adapter help.
4 | Utilities | Reveals the list of In-Sight® Utilities, allowing you to perform configuration, management or maintenance operations on the selected device(s).

Right-clicking on a device in the Device Pane displays a context menu, offering the Create Report option:

Use this option to quickly check the status data of the selected device, such as the name, IP Address, model, and current state of the device.

Note:

When you press the Refresh Devices button above the Device Pane, the following status message and buttons appear while the software is checking for devices on the network:

You can use these buttons to open the Configure Host PC Network Settings Dialog, the Network dialog to add a remote subnet, or refresh the device list.