# Device Addressing – Name

The Name column of the Device Addressing tab shows the name of the data block that can be communicated to or from the Mitsubishi PLC/MC. In-Sight Vision Suite uses four data blocks:

- Control: Used to send control commands (including triggers) to the vision system.
- Status: Used to indicate the status of the vision system.

- Input Block: Used to input application data from the PLC (including parameters for inspection and user data).

- Output Block: Used to output application data to the PLC (including inspection results).

Each block has its own row to configure their starting PLC address by setting a device, its offset, and the number of PLC devices.