# Restart

The Restart utility remotely restarts an In-Sight vision system. Use it as follows:

1. Launch In-Sight Vision Suite if it is not already running.

2. Left-click the device you want to configure on the In-Sight® Device Pane on the left. The list of Utilities applicable to the selected vision system then appears at the bottom of the window.

3. Click the Restart button to launch the Restart Devices utility.

4. The selected device(s) are now displayed. Click the Restart button in the dialog to remotely power cycle the In-Sight vision system (and the devices attached to it, if applicable).