# Set Up the HTTPS Connection

Once you have a valid common Certificate Authority (CA) on the network and the trusted certificates needed to validate the HTTPs connection, you can configure the secure connection to the WebHMI. Depending on the source of the certificates (that is, whether you are using Cognex Network Server or your own custom CA on the network), perform one of the following procedures.