# Camera Configuration

The Camera Configuration utility allows you to configure the resolution for the vision system.

To use the Camera Configuration utility:

1. Launch In-Sight Vision Suite if it is not already running.

2. Left-click the device you want to configure on the In-Sight® Device Pane on the left.

3. The list of Utilities applicable to the selected vision system appears at the bottom of the window. Click Camera Configuration.

   Configure Cameras utility dialog of Camera Configuration opens.

4. Select the resolution that you want to configure from the dropdown list.

5. Click OK.

6. Click Yes to confirm the restart of the device.