# Industrial Ethernet – SLMP Configuration

When the SLMP protocol is selected, the Industrial Ethernet Configuration window changes to display SLMP-specific options:

Configuration options are available in two tabs, Settings and Device Addressing.

Tip: If you configure an incorrect value for a property, the conflicting property or tab is marked in red, and a red exclamation mark appears next to the Restart button at the bottom right of the window. Hover the mouse cursor over the exclamation mark to get more information on the detected error.