# Typical Job Management Sequence

The Current Job ID field module indicates the current job ID of the In-Sight vision system, or 65535 if the current job does not have an ID. In order to load a job, the Automation Controller must set the vision system Offline by using the Set Offline bit. Next, the Command field is set to the desired ID of the job and the Execute Command bit is set. Once the Command Completed bit goes to High, the Execute Command bit is reset.