# Command Result

## Byte 0 - 1

Name | Description
--- | ---
String Command Result Code | The response code for the Native Mode command, which can be used to determine if the command was successful, or failed. Note: Each Native Mode command returns a 1 for a successful execution, while each command has specific error codes for cases of failure. For more information about the failure codes of the individual Native Mode commands, see Native Mode Commands.

## Byte 2 - 3

Name | Description
--- | ---
String Command Result Length | The length of the Response Data of the Native Mode command, in bytes.

## Byte 4 -

Name | Description
--- | ---
String Command Result | The result string of a Native Mode command, an ASCII string representation of the data returned by the command.

Block | Byte | Bit 7 | Bit 6 | Bit 5 | Bit 4 | Bit 3 | Bit 2 | Bit 1 | Bit 0
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
String Command Word | 0..1 | String Command Result Code
2..3 | String Command
4.. | String Command Result Length