# Set Region

Sets an edit region control contained in a cell. The edit region control is always an EditRegion function.

## Set Region Inputs

Syntax: SR<CellName> <X> <Y> <Width> <Height> <Angle> <Curve>

Note: The Set Region command requires a space between all numerical arguments.

Parameter | Description
--- | ---
CellName | The published name of the cell.
Space | A blank space to separate the value from the next value.
Row | The X-offset of the origin, in image coordinates.
Space | A blank space to separate the value from the next value.
Col | The Y-offset of the origin, in image coordinates.
Space | A blank space to separate the value from the next value.
High | The dimension along the X-axis of the region.
Space | A blank space to separate the value from the next value.
Wide | The dimension along the Y-axis of the region.
Space | A blank space to separate the value from the next value.
Angle | The orientation in image coordinates.
Space | A blank space to separate the value from the next value.
Curve | The curvature of the region.

## Set Region Outputs

Returns a status code. The status codes are:

Status Codes | Description
--- | ---
1 | The command was executed successfully.
0 | Unrecognized command.
-1 | The ID is invalid.
-2 | The command could not be executed because the specified cell does not contain an edit region control, or the edit region control was not created by the EditRegion function.
-4 | Wrong argument type.
-6 | User does not have Full Access to execute the command.

## Set Region Example

You can set the Region of an EasyBuilder Location or Inspection Tool by sending a Set Region command containing the position, dimensions, orientation, and shape of the new region.

1. Assume that your job contains an Edge Location Tool, and the region of the tool is currently in another position, with different dimensions, orientation, and shape.

2. To move and re-orient the region settings of the tool through the Set Region Native Mode command, issue the command SREdge_1.Region 192.000 119.000 167.000 20 0.5 0:

3. The In-Sight vision system responds with 1,indicating that the command executed successfully.