# Get Info

Returns the system information for the In-Sight vision system.

## Get Info Inputs

Syntax: GI

## Get Info Outputs

Returns a status code, followed by the system information. The status codes are:

Status Codes | Description
--- | ---
1 | The command was executed successfully.
0 | Unrecognized command.
-2 | The command could not be executed.

The system information includes:

Output | Description
--- | ---
Serial Number | The serial number of the vision system.
Application Version | The current firmware version on the vision system.
Monitor Version | The Monitor version of the vision system. The In-Sight Monitor is used mainly for troubleshooting the In-Sight vision system. Safe Mode allows you to start In-Sight vision system by resetting all the setting parameters. Be aware that this replaces the current settings on the In-Sight vision system, including I/O, startup, and customization, without any prompting or warning. Diagnostics and Server Mode are for internal use and must not be accessed without Cognex technical support assistance. Start In-Sight starts the In-Sight software on the system.
MAC Address | The Media Access Control (MAC) address of the vision system.
Date of Build | The date of the firmware build on the vision system.

## Get Info Example

To display system information about the In-Sight vision system, issue the following command: GI

The In-Sight vision system initially responds with 1, indicating the command successfully executed. On the following lines, the system information is reported.