# Message Functions

Message functions read text strings from an In-Sight vision system and write text strings to an In-Sight vision system over a Native Mode connection.

- ReadMessage: Reads in a text string sent by a remote network host or serial device using the Send Message command.
- WriteMessage: Writes out a text string whenever ReadMessage is executed. WriteMessage outputs the string over the same connection that is used by the ReadMessage function.