# Error ID codes

This table summarizes Error ID codes.

Word | ID code | Description
--- | --- | ---
0x0000 | No Error | No error occurred.
0x0100 | Trigger set while disabled | Occurs when the Trigger bit is set while the Trigger Enable bit is cleared and the Trigger parameter of the AcquireImage function is set to External, Network or Industrial Ethernet.
0x0101 | Trigger set while Offline | Occurs when the Trigger bit is set while the vision system is Offline.
0x0400 | Already Executing Error | Occurs when the Execute Command bit is set and the Executing bit is still High.
0x0401 | Job load requested while Online | Occurs when a Job Load command is issued while the vision system is Online.
0x0402 | Job load requested does not exist on the camera | Occurs when a JobID sent in the Command field does not exist as a prefix for any job in the camera file system. For example, if you send Command = 123, but there is no job on the camera which contains 123xxxxx.job.