# Set Online

Sets the vision system into Online or Offline mode. For more information, see Online and Offline States.

Note:

- This command cannot place the vision system into Online mode if the vision system has been set Offline either manually in the In-Sight user interface, or by a Discrete Input signal.
- The In-Sight 3D Spreadsheet sends Set Online commands to vision systems to perform administrative functions such as Backup and Restore.

## Set Online Inputs

Syntax: SO<Int>

Parameter | Description
--- | ---
Int | 0 = Sets the vision system Offline. 1 = Sets the vision system Online.

## Set Online Outputs

Returns a status code. The status codes are:

Status Codes | Description
--- | ---
1 | The command was executed successfully.
0 | Unrecognized command.
-1 | The value given for Int is either out of range, or is not a valid integer.
-2 | The command could not be executed.
-5 | The communications flag was successful, but the vision system did not go Online because the vision system is set Offline manually through the In-Sight user interface or by a Discrete I/O signal.
-6 | User does not have Full Access to execute the command.

## Example: Set the In-Sight Vision System Into Online Mode

To set the In-Sight vision system into Online mode, issue the following command: SO1

The vision system responds with a status code of 1, indicating that the vision system was successfully placed Online.

## Example: Set the In-Sight Vision System into Offline Mode

To set the In-Sight vision system into Offline mode, issue the following command: SO0

The vision system responds with a status code of 1, indicating that the vision system was successfully taken Offline.