# In-Sight 3800 ビジョンシステム PROFINET IO モジュール参照テーブル

このトピックでは、PROFINET IO モジュール参照テーブルについて説明します。これは、In-Sight ビジョンシステム と Siemens 製 PLC を PROFINET プロトコル経由で組み込むために、GSD ファイルと合わせて使用するものです。

注 : 信号の詳細な説明については、「産業用通信信号」を参照してください。

モジュール | ID | バイト | ビット 7 | ビット 6 | ビット 5 | ビット 4 | ビット 3 | ビット 2 | ビット 1 | ビット 0
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
Acquisition Control | 0x101 | 0 | Set Offline | 予約済み | Clear Exposure Complete | Trigger | Trigger Enable
Acquisition Status | 0x201 | 0 | Online | Offline Reason | Acquisition Error | Exposure Complete | Trigger Acknowledge | Trigger Ready
1 | 予約済み
2 ～ 3 | Acquisition ID
Inspection Control | 0x102 | 0 | Clear Error | 予約済み | Execute Command | Set User Data | Inspection Results Acknowledge | Buffer Results Enable
Inspection Status | 0x203 | 0 | Set User Data Acknowledge | Command Failed | Command Completed | Command Executing | Results Valid | Results Buffer Overrun | Inspection Completed | 予約済み
1 | Error | 予約済み | Job Passed
2 ～ 3 | Error ID
Command Control Input | 0x108 | 0 ～ 1 | Command ID (16 ビット)
Command Control Output | 0x108 | 0 ～ 1 | Current Job ID (16 ビット)
2 ～ 3 | Command Result Code (16 ビット)
Soft Event Control Input | 0x106 | 0 | External Event 7 | External Event 6 | External Event 5 | External Event 4 | External Event 3 | External Event 2 | External Event 1 | External Event 0
External Event Control Output | 0x106 | 0 | External Event Acknowledge 7 | External Event Acknowledge 6 | External Event Acknowledge 5 | External Event Acknowledge 4 | External Event Acknowledge 3 | External Event Acknowledge 2 | External Event Acknowledge 1 | External Event Acknowledge 0
User Data (1016 バイトについて最大 4 モジュール) | 0x301 (16) 0x302 (32) 0x303 (64) 0x304 (128) 0x305 (254) | 0 ～ 1015 (最大) | User Data
Inspection Results (1000 バイトについて最大 4 モジュール) | 0x401 (16) 0x402 (32) 0x403 (64) 0x404 (128) 0x405 (250) | 0 ～ 1 | Inspection ID
2 ～ 3 | Inspection Result Code
4 ～ 1003 (最大) | Inspection Results