# Audit Logging

The Audit Logging utility of In-Sight Vision Suite allows you to track jobs and system level changes and enable traceability and accountability for modifications made to the vision system. To access the Audit Logging utility, you must switch from In-Sight Spreadsheet to the In-Sight Vision Suite application.

The following actions in In-Sight Vision Suite trigger audit logging events:

Changes in the Spreadsheet Editor | System changes | Changing complex tools | Changing utilities
Cell expression Enabling or disabling cell state Symbolic Tag Value change Commenting | From the Sensor Menu: Results Queue Job Status Custom View Discrete IO Online or Offline status change Saving or loading a job | EditCompositeRegion EditFloat EditInt EditMaskedRegion EditMultiGraphics EditPolygon EditPolylinePath EditRegion EditString OCRMax ReadIDMax Script TrainExtractColor TrainPatMaxRedLine ViDiELClassify ViDiELClassify3D ViDiELRead ViDiELSegment ViDiELSegment3D | Connecting to Spreadsheet and EasyBuilder Opening the HMI Audit Logging Backup or Restore Communications settings: Network Settings Host name Serial Configuration Configure SMB Firmware Update HMI Settings Industrial Ethernet IP Licensing License Configuration Restart or Factory Reset Startup Settings User Settings

Note: Audit logging is enabled by default. To download the audit log or enable forwarding, you must have Full user access level privileges. For more information, see User Settings in the In-Sight Vision Suite Software Help document.

To use audit logging:

1. Launch In-Sight Vision Suite if it is not already running.

2. Left-click the vision system you want to configure on the In-Sight® Device Pane on the left. The list of Utilities applicable to the selected vision system then appears at the bottom of the window.

3. Click Audit Logging.

   The Audit Logging window appears.

4. Retrieve the audit log by doing one of the following:

   - Download the audit log by clicking Download.

   - Click Enable Forwarding to enable sending the audit log to a remote server. Set up the IP address and the port number.

     Note: In-Sight Vision Suite uses syslog forwarding protocol to store audit log records. You need to set up a syslog server for collecting audit records.

5. Click OK.