# In-Sight 3800 Vision-System PROFINET IO Modul-Referenztabelle

Dieses Thema enthält die PROFINET IO Modul-Referenztabelle, die zusammen mit der GSD-Datei zur Integration des In-Sight Vision-Systems und einer Siemens-SPS über das PROFINET-Protokoll verwendet werden kann.

Hinweis: Eine ausführliche Beschreibung der Signale finden Sie unter Industrielle Kommunikationssignale.

Modul | ID | Byte | Bit 7 | Bit 6 | Bit 5 | Bit 4 | Bit 3 | Bit 2 | Bit 1 | Bit 0
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
Acquisition Control | 0x101 | 0 | Set Offline | Reserved | Clear Exposure Complete | Trigger | Trigger Enable
Acquisition Status | 0x201 | 0 | Online | Offline Reason | Acquisition Error | Exposure Complete | Trigger Acknowledge | Trigger Ready
1 | Reserved
2..3 | Acquisition ID
Inspection Control | 0x102 | 0 | Clear Error | Reserved | Execute Command | Set User Data | Inspection Results Acknowledge | Buffer Results Enable
Inspection Status | 0x203 | 0 | Set User Data Acknowledge | Command Failed | Command Completed | Command Executing | Results Valid | Results Buffer Overrun | Inspection Completed | Reserved
1 | Error | Reserved | Job Passed
2..3 | Error ID
Command Control Input | 0x108 | 0..1 | Command ID (16 Bit)
Command Control Output | 0x108 | 0..1 | Current Job ID (16 Bit)
2..3 | Command Result Code (16 Bit)
Soft Event Control Input | 0x106 | 0 | External Event 7 | External Event 6 | External Event 5 | External Event 4 | External Event 3 | External Event 2 | External Event 1 | External Event 0
External Event Control Output | 0x106 | 0 | External Event Acknowledge 7 | External Event Acknowledge 6 | External Event Acknowledge 5 | External Event Acknowledge 4 | External Event Acknowledge 3 | External Event Acknowledge 2 | External Event Acknowledge 1 | External Event Acknowledge 0
User Data (bis zu 4 Module für 1016 Byte) | 0x301 (16) 0x302 (32) 0x303 (64) 0x304 (128) 0x305 (254) | 0..1015 max | User Data
Inspection Results (bis zu 4 Module für 1000 Byte) | 0x401 (16) 0x402 (32) 0x403 (64) 0x404 (128) 0x405 (250) | 0..1 | Inspektions-ID
2..3 | Inspection Results Code
4..1003 max | Inspection Results