# WriteResultsBuffer

Writes data from a referenced Buffer data structure, created by a FormatOutputBuffer function Functions are tools that are available in Spreadsheet for processing and analyzing acquisitions or other results. You can add functions to your Spreadsheet job to create tool chains and produce results for specific applications., to the currently enabled factory communication protocol. This function also writes the Result Code field for the factory communication protocols.

Inputs

Parameter | Description
Event | Specifies the event that forces an update. This parameter needs to be a reference to any event with a timestamp, for example, one of the following: A cell containing an Event function. A cell containing a Button function.
Inspection ID | If the function references a cell pointing to a PointCloud A point cloud is a 3D structure that consists of the data points collected by a 3D vision system during acquisition. structure (default = A0), the Inspection ID of the result is the Acquisition Acquisition is the process or result of the vision system acquiring a new image. ID of the hardware acquisition that produced the result, or -1=0xFFFF if the PointCloud does not come from a hardware acquisition. If the function references a cell with an integer value, the Inspection ID of the result is set to that value.
Buffer | Specifies a reference to a Buffer data structure created by a FormatOutputBuffer function, which contains automatically formatted data.
Result Code | Specifies an integer that can be used to communicate the result of the inspection to any connected devices.
Protocol | Specifies which protocol the user data needs to be written to.
1 = EtherNet/IP | Specifies that EtherNet/IP is the enabled factory communication protocol.
2 = PROFINET | Specifies that PROFINET is the enabled factory communication protocol.
3 = SLMP Protocol Scanner | Specifies that SLMP is the enabled factory communication protocol.
4 = Modbus TCP Server | Specifies that Modbus TCP is the enabled factory communication protocol.
100 = Default | Specifies that the currently enabled factory communication protocol is used. If more than one protocol is enabled, the first enabled protocol is used.
Byte/Word Order | Specifies the bit order for words and bytes read by the function.
0 = Big endian | Specifies that the most significant byte is stored first and subsequent bytes are stored in descending order.
1 = Little endian | Specifies that the least significant byte is stored first and subsequent bytes are stored in ascending order.
2 = Big endian with 16-bit word swapping | Big endian byte style is applied and double word types have their word pair order switched. (16-bit words)
3 = Little endian with 16-bit word swapping | Little endian byte style is applied and double word types have their word pair order switched. (16-bit words)
100 = Default | The default setting is used.

Outputs

Returns | A Write Result data structure containing the data sent to the client, or #ERR: If an input parameter is invalid If a connection to a client has not been established