# DelayLine

Implements a shift-register array, or data "stream", into which a cell's values are buffered after each event.

Note: After a reset, the first value that is read fills the shift-register.

## DelayLine Inputs

Syntax: DelayLine(Event,Value,Number of Steps,Reset)

Parameter | Description
--- | ---
Event | Specifies the event that forces an update.This parameter must be a reference to one of the following: The Image data structure in cell A1. A cell containing an Event function Functions are tools that are available in Spreadsheet for processing and analyzing acquisitions or other results. You can add functions to your Spreadsheet job to create tool chains and produce results for specific applications.. A cell containing a Button function. Note: DelayLine buffers the state of a referenced value before that value is updated by any other function that depends on the specified Event.
Value | A reference to the cell containing the source data (-16777216 to 16777216; default = 0).
Number of Steps | Specifies the number of values in the function's internal shift-register array. (default = 10)
Reset | Forces the function to purge itself of previously read values. The first value read after Reset will effectively "fill" the shift register.
0 = OFF (default) | The function will continue to read in values to the data stream.
1 = ON | The function will purge all values from the data stream.

## DelayLine Outputs

Returns | A Delay data structure containing statistics for the specified Value over an interval from Reset to current.
Results | When the function initially inserted into a cell, a result table is created in the spreadsheet.

## DelayLine Vision Data Access Functions

The following Vision Data Access functions are automatically inserted into the spreadsheet to create the result table.

Last | GetValue(Delay, Index) | The last value contained in the structure.
Mean | GetMean(Delay) | The mean of all the values in the structure.
SDev | GetSDev(Delay) | The standard deviation of all the values in the structure.
Min | GetMin(Delay) | The smallest value contained in the structure.
Max | GetMax(Delay) | The largest value contained in the structure.

Additional data elements can be accessed using the following Vision Data Access functions:

Count | GetCount(Delay) | The number of values contained in the structure.
Sum | GetSum(Delay) | The sum of all values contained in the structure.