# SLMP Cyclic Connection Times Support

SLMP supports the following cyclic connection times (or poll intervals) and data amount to be sent with a cyclic connection:

- Cycle times of cyclic connections can be 5 – 30000 ms.

- User data and inspection result size within a cyclic connection depends on the type of PLC A Programmable Logic Controller is a ruggedized computer that you can use for automating processes or even an entire production line./MC used:

  - In case of Mitsubishi iQ-Q Series: Up to 960 words (15360 bits), or 3584 bits for bit devices.

  - In case of Mitsubishi FX Series: Up to 64 words (1024 bits), or 256 bits for bit devices.