Note: In-Sight supports TLS versions 1.2 and 1.3 for HTTPS communication.

1. Click Certificate Signing Request... to create a CSR for your vision system.

2. In the Certificate Signing Request dialog that opens, populate the fields as follows:

   Field | Description
   --- | ---
   Country Code | The two-letter ISO code for the country where your organization is located.
   State | The name of the province, region, county, or state in which your organization is located.
   Locality | The name of the town, city, village, or other administrative unit in which your organization is located.
   Company | The legal name of your company, including any suffixes such as Ltd. or Corp.
   Organizational Unit | The name of your department or division within the company.
   Common Name | The main IP address of the vision system.
   Subject Alternative Name | Any additional fully qualified domain names that you want to secure. Values must be prefixed by DNS: or IP: depending on the value. For vision systems with multiple Ethernet interfaces, provide an entry for both IP addresses. You can provide multiple entries by separating them with either a comma or a line break.

   Click Submit to create a .csr file.

3. Submit the .csr file to your Certificate Authority (CA) for signing according to the designated CA process within your organization. Once the CA validates your request, you receive a signed certificate file with a .crt, .cer, or .pem extension.

4. After you have received your certificate file, return to the main Configure Secure Connection dialog, and click Import Certificate.

5. In the file browser that opens, select the certificate file that you received from your CA, and click Open.

   The Configure Secure Connection dialog now displays the details of your current certificate:

   All HTTPS traffic to and from the vision system now uses the installed certificate.