# WriteDevice

Exports data from the In-Sight vision system to another host on the network using a TCP/IP connection.

Note: The WriteDevice function Functions are tools that are available in Spreadsheet for processing and analyzing acquisitions or other results. You can add functions to your Spreadsheet job to create tool chains and produce results for specific applications. can send a message to a remote host while either Online or Offline.
Inputs

Parameter | Description
Event | Specifies the event that forces an update. This parameter must be a reference to one of the following: The Image data structure in cell A0, containing the AcquireImage function. For more information, see . A cell containing an Event function. For more information, see Event. A cell containing a Button function. For more information, see Button.
Device | A reference to a spreadsheet cell containing a Device data structure created by a TCPClient or a TCPServer function. If the Spreadhsheet cell contains a TCPClient function and the connection is not yet established, the Event update triggers a reconnection attempt. For more information, see TCPClient.
Data 1, 2, ... | A reference to a cell which contains the data to export to the TCP/IP server device specified in the TCPClient function. Multiple data inputs are concatenated in a single packet.

Outputs

Returns | A Write data structure, containing the data that is exported whenever the specified Event is initiated, or #ERR if there is any error: Any of the input parameters are invalid. For a TCPClient device, reports if a connection could not be established during the timeout period. For a TCPServer device, reports if there is no connection available.