# Result Queue

The Result Queue creates a filmstrip on the WebHMI The operator interface through which the operator interacts with the vision system. about the results.

Results Queue Settings:

Number | Element | Description
1 | Enable result queue | Enables/disables the result queue in the WebHMI. The default setting is disabled.
2 | Mode | Sets what kind of results show up on the result queue. You can choose from the following: Pass and Fail Results Fail Results Pass Results Separate Pass and Fail Results The default setting is Pass and Fail Results.
3 | Queue Size | Sets the queue size, which means how many results you can see in the result queue. The default value is 10 results.
4 | Pass Size | Sets the queue size, which means how many pass results you can see in the result queue. The default value is 1 results.
5 | Fail Size | Sets the queue size, which means how many fail results you can see in the result queue. The default value is 9 results.
6 | Queue offline results | Enables/disables to queue the offline results.
7 | Keep first results | Enables/disables keeping the first results in the result queue.
8 | Clear when placed in online mode | Clears the result queue when you set the vision system to online mode.
9 | Result Condition | Conditions the result queue. Click Select Cell to watch that cell. You can condition the cell watching with the following options: Fail cell with #ERR Fail cell with value < 0 Fail cell with value = 0 Fail cell with value > 0

To add a Result Queue:

1. Navigate to Sensor menu and select Result Queue Settings.

2. Enable the Enable result queue checkbox.

3. Adjust your settings and click OK.