# Time/Timer Vision Data Access functions

This topic lists the Vision Data Access functions that report execution cell times, read date and time from an internal clock, and trigger an event after a specified interval or at specified times. The GetScanTime function Functions are tools that are available in Spreadsheet for processing and analyzing acquisitions or other results. You can add functions to your Spreadsheet job to create tool chains and produce results for specific applications. is related to the functions described in this topic.

Note: All returned values are from a referenced function or cell.

Function | Description
--- | ---
GetAllTime(Image) | Returns the time in milliseconds from the start of an image acquisition Acquisition is the process or result of the vision system acquiring a new image. to the end of a job A job is a user-configured program in Spreadsheet consisting of functions and designed for specific applications. You can create and edit jobs using the Spreadsheet interface, and load them on a vision system for deployment in a live environment. execution, or #ERR if the input value is invalid. Note: If the vision system is offline, the returned value is higher than when the vision system is online. When the vision system is offline, it takes additional steps that allow the user to modify the filters after making the acquisition.
GetTime(Cell1, [Cell2, ...]) | Returns the time in milliseconds for a variable-length list of cells to execute or #ERR if the input value is invalid. If multiple cells are selected, the sum of all execution times is returned. In addition, you can use the function to returns the acquisition time in milliseconds from when the CPU receives the first laser profile until the full point cloud A point cloud is a 3D structure that consists of the data points collected by a 3D vision system during acquisition. is generated.