# EtherNet/IP Input Assembly - Instance 13

Note: For detailed descriptions of the signals, see Industrial Communications Signals.

Instance | Byte | Bit 7 | Bit 6 | Bit 5 | Bit 4 | Bit 3 | Bit 2 | Bit 1 | Bit 0
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
13 | 0 | Online | OfflineReason | Acq Error | Reserved | Trigger Ack | Trigger Ready
1 | Error | Command Failed | Command Completed | Command Executing | Results Valid | Results Buffer Overrun | Inspection Completed | Reserved
2 | Reserved | SystemValidated | JobPass | Exposure Complete | Reserved | Set User Data Acknowledge
3 | External Event Acknowledge 7 | External Event Acknowledge 6 | External Event Acknowledge 5 | External Event Acknowledge 4 | External Event Acknowledge 3 | External Event Acknowledge 2 | External Event Acknowledge 1 | External Event Acknowledge 0
4 .. 5 | Error ID (16-bit integer)
6 .. 7 | Command Result Code (16-bit integer)
8 .. 9 | Current Job A job is a user-configured program in In-Sight Spreadsheet consisting of functions and designed for specific applications. You can create and edit jobs using the In-Sight Spreadsheet interface, and load them on a vision system for deployment in a live environment. ID (16-bit integer)
10 .. 11 | Acquisition Acquisition is the process or result of the vision system acquiring a new image. ID (16-bit integer)
12 .. 13 | Inspection ID (16-bit integer)
14 .. 15 | Inspection Result Code (16-bit integer)
16 .. 499 | Inspection Results 0 - 483
16 | Inspection Results 0
... |
499 | Inspection Results 483