# TransFixtureToPixel

Converts a point in Fixture coordinates to Pixel coordinates.

## TransFixtureToPixel Inputs

Parameter | Description
Fixture | Specifies the fixture coordinate system.
X | Offset from image X origin.
Y | Offset from image Y origin.
Theta | The rotation from the image X axis, in the image coordinate system. (+/-360 degrees clockwise)
Point | Specifies the coordinates of the point, in fixture coordinates.
X | X offset of the point from the fixture origin.
Y | Y offset of the point from the fixture origin.
Show | Specifies the display mode for the TransFixtureToPixel graphic overlay on the image.
0 = hide all (default) | The point will not be displayed, unless the cell containing the TransFixtureToPixel function is highlighted in the spreadsheet.
1 = result graphics only | The point will always be displayed.

## TransFixtureToPixel Outputs

Returns | A Point data structure containing the transformed point, or #ERR if any of the input parameters are invalid.
Results | When the function is initially inserted into a cell, a result table is created in the spreadsheet.

## TransFixtureToPixel Vision Data Access Functions

The following Structures Vision Data Access functions are automatically inserted into the spreadsheet to create the results table:

Label | Function | Description
--- | --- | ---
X | GetX(Point) | The X-coordinate of the transformed point.
Y | GetY(Point) | The Y-coordinate of the transformed point.