# Adding the In-Sight Vision System to the HW Configuration

By performing the procedure of Importing the GSD File into the Catalog, the In-Sight vision system should appear in the Catalog on the right side of the window.

Once the vision system is found, perform the following steps to add it to the HW Config:

1. Drag and drop In-Sight Vision System to the PROFINET-IO-System of the HW Config.

2. Right-click on the PROFINET-IO-System and select Object Properties. Uncheck the Use name in IO device / controller setting if it is checked, then click OK.

3. Right-click on the In-Sight vision system in the HW Config, then select Object Properties. Type the same name for Device name that was configured for Station Name in In-Sight Vision Suite in Step 5 of Setting up the In-Sight Vision System.

Note:

If the Assign IP address via IO controller option is unchecked, the system keeps the IP address of the vision system. If it is checked, its IP address is changed to a value provided by the CPU.