# Put Live

Turns live acquisition mode ON or OFF.

Note: The vision system must be Offline.

## Put Live Inputs

Syntax:[Put Live][Int]

Parameter | Description
--- | ---
Int | 0 = Disable live acquisition mode. 1 = Enable live acquisition mode.

## Put Live Outputs

Returns a status code. The status codes are:

Status Codes | Description
--- | ---
1 | The command was executed successfully.
0 | Unrecognized command.
-1 | The input is invalid or has exceeded 15 bytes in length.
-2 | The command could not be executed, or the vision system is Online.
-6 | User does not have Full Access to execute the command.

## Put Live Examples

To place the vision system into live acquisition mode, issue the following command: Put Live 1

The In-Sight vision system responded with a status code of 1, indicating that the vision system was successfully placed into live acquisition mode.

To take the vision system out of live acquisition mode, issue the command: Put Live 0

The vision system responded with a status code of 1, indicating that the vision system was successfully taken out of live acquisition mode.