# Get FileList

Returns the number of files stored in memory, and the name of each file in memory on theIn-Sightvision system.

Note:

- If a RAM Disk folder is enabled on the vision system, the "RAMDisk" folder name is included in the Get Filelist output.
- It is not possible to get the file list from a RAM Disk folder using the Get Filelist Native Mode command. In order to obtain the file list of a RAM Disk folder, use the FTP protocol instead. Note that the CD (change directory) FTP command is not supported.

## Get FileList Inputs

Syntax: Get FileList

## Get FileList Outputs

A status code, followed by the number of files stored in memory, followed by the name of each file in memory. The status codes are:

Status Codes | Description
--- | ---
1 | The command was executed successfully.
0 | Unrecognized command.
-1 | The input is invalid or has exceeded 15 bytes in length.
-2 | The command could not be executed.

## Get FileList Example

To retrieve a count and list of files that are stored on the In-Sightvision system, issue the following command: Get FileList

The vision system responds with a status code (1), followed by the number of files present in memory (13). Finally, the individual name of each file is displayed.