# Reset (Reboot)

Resets the In-Sight vision system. This command is similar to physically cycling power on the vision system.

## Reset (Reboot) Inputs

Syntax: RT

## Reset (Reboot) Outputs

Returns a status code, followed by a line terminator, followed by lines of settings data. The only status code returned is

Status Codes | Description
--- | ---
-6 | User does not have Full Access to execute the command.

## Reset System Example

To reset the In-Sight vision system, issue the following command: RT

The In-Sight vision system is successfully reset and no status code is returned.