# Known Issues

Issue # | Known Issue
--- | ---
IS280-628 | Date/timestamps from the vision system is set to the time of manufacture, not to the current date/time.
IS280-892 | Having the editor connected to a vision system while online affects job performance. Make sure that an editor is not connected to an online vision systemunless it is in a state where the job performance is not critical.
ISPROD-971 | Delayed response when working on a job with lots of cells.
IS280-10296 | There is a one-second time frame during firmware update when the power loss happens. To avoid this, do not disconnect power during firmware update.
IS280-10985 | If you link a tool to the Communication application step property and then you delete, the links to that tool in the Communication application step gets removed. If you perform an undo of that deletion then the tool is present again, but the links to the tool are not reestablished in the Communication application step. The only exception are the links on the right side of the screen such as context panel where the "enabled" link is restored.
N/A | If using OPCUA with the network settings set to DHCP instead of static IP, occasional loss of connection happens. To avoid this, use a static IP address.
ISPROD-1330 | When you fixture a pattern tool to another pattern tool, the tool location moves properly with the fixture. However, the angle does not. The angle range appears to reference the main image and not the fixture.
ISPROD-2160 | Emoji or Unicode password characters are not supported, but are occasionally allowed.
ISPROD-3869 | WriteImage does not create subfolders on the FTP server and will fail to transfer if they do not already exist. To avoid this, ensure that the directories exist before attempting to write to them via FTP.
ISPROD-3996 | ReadIDMax does not support Kanji output with GetStringIDMax.
ISPROD-4320 | SVGs and images with graphics are clipped incorrectly if browser scaling is enabled.
ISPROD-4705 | A .bmp image saved from one In-Sight 2800 sensor is unable to open on another In-Sight 2800 camera
ISPROD-5485 | Attempting to connect to both instances of a dual ethernet vision system by selecting both and then clicking on a connect option in ISVS reboots the sensor. The sensor needs to be physically power cycled.
ISPROD-6455 | Find Pattern default search ROI is out of bounds when the acquire start row is greater than 0.
ISPROD-6585 | After linking a property in In-Sight, values cannot be updated before the trigger.
ISPROD-7521 | Issues with the image border on the HDR+.
ISPROD-8482 | The white balance default is discolored.
ISPROD-8923 | A job with many EL tools fails to load due to a UI timeout.
ISPROD-8946 | Unable edit CalibrateGrid cell when there is an insufficient number of calibration points error. When there is insufficient detection of points in a region, the CalibrationGrid cell function can end up in an irrecoverable state. There is no way to recover from this state other than deleting the CalibrationGrid cell. If recalibration is mistakenly performed while existing calibration data is present, there is a risk of losing the existing calibration data. However, reloading the job if it is saved can help recover the data.
ISPROD-9160 | There is a delay in the output timing of the Acquisition Start signal, which causes a mismatch with the strobe signal. While the Acquisition Start signal is not commonly used in actual control, it is important to be aware that there might be a discrepancy with the strobe signal.
ISPROD-9023 | Apply Immediately in ApplyAcquisitionSettings is not functioning as expected. Illumination properties ignore the Apply Immediately setting. Illumination property changes are always reflected on the next acquisition.