# Get Info

Returns the system information for the In-Sightvision system.

## Get Info Inputs

Syntax: GI

## Get Info Outputs

Returns a status code, followed by the system information.

The status codes are:

Status Codes | Description
--- | ---
1 | The command was executed successfully.
0 | Unrecognized command.
-2 | The command could not be executed.

The system information includes:

Output | Description
--- | ---
Serial Number | The serial number of the Vision System.
Application Version | The current firmware version on the Vision System.
Monitor Version | The Monitor version of the Vision System. The In-Sight Monitor is used mainly for troubleshooting the In-Sight sensor. "Safe Mode" allows you to start In-Sight by resetting all the setting parameters; be aware that this will replace the current "Settings" on the In-Sight sensor, including I/O, startup, and customization, without any prompting or warning. "Diagnostics" and "Server Mode" are for internal use and should not be accessed without Cognex technical support assistance. "Start In-Sight" starts the In-Sight software on the system.
MAC Address | The Media Access Control (MAC) address of the Vision System.
Date of Build | The date of build of the firmware on the Vision System.

## Get Info Example

To display system information about the In-Sightvision system, issue the following command: GI

The In-Sightvision system initially responds with 1, indicating the command successfully executed. On the following lines, the system information is reported.