# Checking the Application

Once you configured the job in the In-Sight adapter, the Online Enabled and Online Enable Comm bits need to have a value of true in SIMATIC Manager while the job is running on the In-Sight vision system.

To trigger the In-Sight vision system, perform the following steps:

1. Enable the Trigger Enable bit by setting this bit to true in the Modify value column, then click Activate modify values. The bit then needs to become true, indicating that the vision system is ready to be triggered.

2. Trigger the vision system by giving it a rising edge on . “Rising edge” means that the bit is first set to true (by setting it to true in the Modify value row and clicking on the Activate modify values icon), and then set back to false.

   When the bit is set to true, the and bits need to also change to true, indicating that triggering is completed. The value increments each time the PLC triggers the camera.

   Likewise, once is set back to false, the bit also changes to false again.

3. Check the job; the newly-acquired image needs to appear.